# Data Object - VMwareDVSVlanMtuHealthCheckConfig(vim.dvs.VmwareDistributedVirtualSwitch.VlanMtuHealthCheckConfig)

Extends
  VMwareDVSHealthCheckConfig
Since
  vSphere API 5.1

## Data Object Description

This class defines the vlan and mtu health check configuration. Vlan health check is used to check whether vlans are trunked by the physical switch connected to the uplink ports. MTU health check is used to verify current MTU setting workable on all uplink ports of the vSphere Distributed Switch.

Properties

Name | Type | Description
--- | --- | ---
None
Properties inherited from VMwareDVSHealthCheckConfig
None
Properties inherited from DVSHealthCheckConfig
enable, interval
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sms="urn:sms" name="VMwareDVSVlanMtuHealthCheckConfig"> <complexContent> <extension base="sms:VMwareDVSHealthCheckConfig"> <sequence> </sequence> </extension> </complexContent> </complexType>