# Data Object - VsanHostIpConfig(vim.vsan.host.IpConfig)

Property of
  VsanHostConfigInfoNetworkInfoPortConfig
Extends
  DynamicData
Since
  vSphere API 5.5

## Data Object Description

An VsanHostIpConfig is a pair of multicast IP addresses for use by the VSAN service. For VSAN there is one such IpConfig pair per "virtual network" as represented by VsanHostConfigInfoNetworkInfoPortConfig.
See VsanHostConfigInfoNetworkInfo
See port
See VsanHostConfigInfoNetworkInfoPortConfig
See UpdateVsan_Task

Properties

Name | Type | Description
--- | --- | ---
downstreamIpAddress | xsd:string | Master-to-agent multicast IP address.
upstreamIpAddress | xsd:string | Agent-to-master multicast IP address.
Properties inherited from DynamicData
None

Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sms="urn:sms" name="VsanHostIpConfig"> <complexContent> <extension base="sms:DynamicData"> <sequence> <element name="upstreamIpAddress" type="xsd:string"/> <element name="downstreamIpAddress" type="xsd:string"/> </sequence> </extension> </complexContent> </complexType>