# Enum - HostNumericSensorHealthState(vim.host.NumericSensorInfo.HealthState)

Since
  VI API 2.5

## Enum Description

Health state of the numeric sensor as reported by the sensor probes. Same data reported using command line: esxcli hardware ipmi sdr list

Enum Constants

Name | Description
--- | ---
green | The sensor is operating under normal conditions
red | The sensor is operating under critical or fatal conditions. This may directly affect the functioning of both the sensor and related components.
unknown | The implementation cannot report on the current health state of the physical element
yellow | The sensor is operating under conditions that are non-critical.

Show WSDL type definition
<simpleType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sms="urn:sms" name="HostNumericSensorHealthState"> <restriction base="xsd:string"> <enumeration value="unknown"/> <enumeration value="green"/> <enumeration value="yellow"/> <enumeration value="red"/> </restriction> </simpleType>