# Data Object - HostMultipathInfo(vim.host.MultipathInfo)

Property of
  HostStorageDeviceInfo
Extends
  DynamicData
See also
  HostMultipathInfoLogicalUnit

## Data Object Description

The HostMultipathInfo data object describes the multipathing policy configuration to determine the storage failover policies for a SCSI logical unit. The multipathing policy configuration operates on SCSI logical units and the paths to the logical units.

Multipath policy configuration is only possible on storage devices provided by the native multipathing plug-store plugin. Storage devices using the native multipathing storage plugin will have an entry in this data object. Storage devices provided by a different storage plugin will not appear in the inventory represented by this data object.

Legacy note: In hosts where HostMultipathStateInfo is not defined or does not exist on the HostStorageDeviceInfo object, only native multipathing exists. That means for these hosts, the MultipathInfo object contains the complete set of LUNs and paths on the LUNs available on the host.

Properties

Name | Type | Description
--- | --- | ---
lun* | HostMultipathInfoLogicalUnit[] | List of logical units that can be configured for multipathing.
Properties inherited from DynamicData
None

*Need not be set
Show WSDL type definition
<complexType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:pbm="urn:pbm" name="HostMultipathInfo"> <complexContent> <extension base="pbm:DynamicData"> <sequence> <element name="lun" type="pbm:HostMultipathInfoLogicalUnit" minOccurs="0" maxOccurs="unbounded"/> </sequence> </extension> </complexContent> </complexType>